
**Re-Flash inverter SOP**


1. Connect PC and inverter device with serial cable. Only through the RS232 port update.




1. Run ReflashTool.exe as below.




1. Choose valid serial port which connect to inverter device.



1. Click ”Update DSP” button and wait for 15 seconds to update DSP.



1. When update DSP completed, click ”Update MCU” and wait for 15 seconds to update MCU.



1. If the LCD display 17 error, click ”Rest EEPROM”。 Otherwise ignore this step.

